**BECA**

**Project Details:**

* Requires AutoCAD 2018
* Developed in C# language

**To Setup BECA in AutoCAD 2018:**

* We need “B-Civil.cuix” file. It should be in the path - “C:\BECA\B-Civil.cuix”. For that paste “BECA” folder and paste it in “C:\”.
* We need required drawings to load signs in autocad. The drawings should be in the path –

“C:\Users\Public\Documents\BecaCAD\Autodesk\ACAD2018\Symbols\CIVIL\NZ\NZTA Signs”.

For that paste “BecaCAD” folder and paste it in “C:\Users\Public\Documents\”.

* Also we need “B-Civil.xml” file to filter the drawings. It should be in the path -

“C:\Users\Public\Documents\BecaCAD\Autodesk\ACAD2018\Symbols\CIVIL\NZ\NZTA Signs”.

For that paste “BecaCAD” folder and paste it in “C:\Users\Public\Documents\”.

**To run BECA in AutoCAD 2018:**

* First we need to load the “B-Civil.cuix” file in AutoCAD 2018.
* Run **“CUI”** command.
* In Customize User Interface dialog, click Open button.
* In Open dialog, select “B-Civil.cuix” file path and click Open button.
* Load required dll files using **“NETLOAD”** command.